IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "/dev/null"
Time stamp: "2026-05-28T17:27:22+02:00"
Preprocessor: "IfcOpenShell 0.8.5"
Originating system: "IfcOpenShell 0.8.5"
Authorization: "Nobody"

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE

Spatial structure
IFCPROJECT "PIM-INSULATION-CELLULOSE-TEXTILE-001"
  IFCSITE "Site"
    IFCBUILDING "Building"
      IFCBUILDINGSTOREY "Storey 0"
        contains 1 element
          1 x IFCCOVERING | INSULATION | names: "Aislante celulósico/textil reciclado" | descriptions: "Manto/panel aislante mixto celulosa+fibra textil para cámara de tabiquería seca y techos. Datos pre-lab estimados desde Isocell, Climacell, Métisse EPDs públicas." | material: "recovered cellulose fibers" | property sets: Pset_Recycled_Source, Pset_Recycled_Content, Pset_Recycled_Fire, Pset_Recycled_Thermal, Pset_Recycled_Acoustic, Pset_CoveringCommon

Property sets
  Pset_Recycled_Source | properties | on 1 object (1 IFCCOVERING)
    DataConfidence = 0 (IFCINTEGER)
    LastUpdated = "2026-05-28" (IFCLABEL)
    ProductVersion = "0.2.1" (IFCLABEL)
    SKU = "INSULATION-CELLULOSE-TEXTILE-001" (IFCLABEL)
    TechnicalSheetURL = "" (IFCLABEL)
  Pset_Recycled_Content | properties | on 1 object (1 IFCCOVERING)
    ContentMethodology = "ISO 14021 self-declaration (pending verification)" (IFCLABEL)
    RecycledContentPercent = 85. (IFCREAL)
    WasteSource = "post_consumer_paper_cardboard, post_consumer_textile_collection" (IFCLABEL)
  Pset_Recycled_Fire | properties | on 1 object (1 IFCCOVERING)
    DropletsClass = "not_declared" (IFCLABEL)
    FireClassEN13501_1 = "E" (IFCLABEL)
    FireTestReportId = "LIT-REF-v0.2-2026-05-20" (IFCLABEL)
    SmokeClass = "not_declared" (IFCLABEL)
  Pset_Recycled_Thermal | properties | on 1 object (1 IFCCOVERING)
    ThermalConductivity = 0.040000000000000001 (IFCREAL)
    ThermalTestMethod = "EN 12667 / EN 12939 (literature reference, Isocell/Climacell/Métisse EPDs)" (IFCLABEL)
    ThermalTestReportId = "LIT-REF-v0.2-2026-05-20" (IFCLABEL)
  Pset_Recycled_Acoustic | properties | on 1 object (1 IFCCOVERING)
    AcousticTestReportId = "LIT-REF-v0.2-2026-05-20" (IFCLABEL)
    AlphaW = 0.90000000000000002 (IFCREAL)
    TestMethodAcoustic = "EN ISO 354 + EN ISO 11654 (literature reference, aislantes semirrígidos 60 mm en cámara)" (IFCLABEL)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Combustible = TRUE (IFCBOOLEAN)
    FireRating = "E" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "INSULATION-CELLULOSE-TEXTILE-001" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCCOVERING)
    ArticleNumber = "INSULATION-CELLULOSE-TEXTILE-001" (IFCIDENTIFIER)
    AssemblyPlace = "ES" (IFCLABEL)
    Manufacturer = "RecycleBIM" (IFCLABEL)
    ProductionYear = "2026" (IFCLABEL)
  Pset_Recycled_EnvironmentalImpact | properties | on 1 object (1 IFCCOVERING)
    BiogenicCarbon_kgCO2_per_kg = -0.34999999999999998 (IFCREAL)
    DeclaredValueType = "estimated_literature" (IFCLABEL)
    EPDStatus = "literature_estimate" (IFCLABEL)
    EmbodiedEnergy_MJ_per_kg = 4.7999999999999998 (IFCREAL)
    GWP_kgCO2eq_per_kg = 0.41999999999999998 (IFCREAL)
    LCAModuleCoverage = "A1-A3" (IFCLABEL)
  Pset_Recycled_Hygrothermal | properties | on 1 object (1 IFCCOVERING)
    Porosity_percent = 90. (IFCREAL)
    SpecificHeatCapacity_J_per_kg_K = 1700. (IFCREAL)
    VapourDiffusionResistanceFactor_mu = 1.5 (IFCREAL)
  Pset_Recycled_Classifications | properties | on 1 object (1 IFCCOVERING)
    OmniClass_Code = "23-15 11 11" (IFCLABEL)
    OmniClass_Table = "23" (IFCLABEL)
    OmniClass_Title = "Building Insulation, Thermal" (IFCLABEL)
    Uniclass2015_Code = "Pr_25_71_50" (IFCLABEL)
    Uniclass2015_Table = "Pr" (IFCLABEL)
    Uniclass2015_Title = "Insulation, thermal and acoustic" (IFCLABEL)