IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "/dev/null"
Time stamp: "2026-05-28T17:27:22+02:00"
Preprocessor: "IfcOpenShell 0.8.5"
Originating system: "IfcOpenShell 0.8.5"
Authorization: "Nobody"

Units
  VOLUMEUNIT: CUBIC_METRE
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE

Spatial structure
IFCPROJECT "PIM-PANEL-ACOUSTIC-TEXTILE-001"
  IFCSITE "Site"
    IFCBUILDING "Building"
      IFCBUILDINGSTOREY "Storey 0"
        contains 1 element
          1 x IFCCOVERING | CLADDING | names: "Panel acústico interior textil reciclado" | descriptions: "Panel acústico decorativo para interior fabricado con fibras textiles recuperadas post-consumo. Valores técnicos pre-lab estimados a partir de productos análogos (Métisse®, Buitex, EconitTM)." | material: "cotton/polyester recovered fibers" | property sets: Pset_Recycled_Source, Pset_Recycled_Content, Pset_Recycled_Fire, Pset_Recycled_Thermal, Pset_Recycled_Acoustic, Pset_CoveringCommon

Property sets
  Pset_Recycled_Source | properties | on 1 object (1 IFCCOVERING)
    DataConfidence = 0 (IFCINTEGER)
    LastUpdated = "2026-05-28" (IFCLABEL)
    ProductVersion = "0.2.1" (IFCLABEL)
    SKU = "PANEL-ACOUSTIC-TEXTILE-001" (IFCLABEL)
    TechnicalSheetURL = "" (IFCLABEL)
  Pset_Recycled_Content | properties | on 1 object (1 IFCCOVERING)
    ContentMethodology = "ISO 14021 self-declaration (pending verification)" (IFCLABEL)
    RecycledContentPercent = 80. (IFCREAL)
    WasteSource = "post_consumer_textile_collection" (IFCLABEL)
  Pset_Recycled_Fire | properties | on 1 object (1 IFCCOVERING)
    DropletsClass = "not_declared" (IFCLABEL)
    FireClassEN13501_1 = "E" (IFCLABEL)
    FireTestReportId = "LIT-REF-v0.2-2026-05-20" (IFCLABEL)
    SmokeClass = "not_declared" (IFCLABEL)
  Pset_Recycled_Thermal | properties | on 1 object (1 IFCCOVERING)
    ThermalConductivity = 0.044999999999999998 (IFCREAL)
    ThermalTestMethod = "EN 12667 (literature reference)" (IFCLABEL)
    ThermalTestReportId = "LIT-REF-v0.2-2026-05-20" (IFCLABEL)
  Pset_Recycled_Acoustic | properties | on 1 object (1 IFCCOVERING)
    AcousticTestReportId = "LIT-REF-v0.2-2026-05-20" (IFCLABEL)
    AlphaW = 0.80000000000000004 (IFCREAL)
    TestMethodAcoustic = "EN ISO 354 + EN ISO 11654 (literature reference)" (IFCLABEL)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Combustible = TRUE (IFCBOOLEAN)
    FireRating = "E" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "PANEL-ACOUSTIC-TEXTILE-001" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCCOVERING)
    ArticleNumber = "PANEL-ACOUSTIC-TEXTILE-001" (IFCIDENTIFIER)
    AssemblyPlace = "ES" (IFCLABEL)
    Manufacturer = "RecycleBIM" (IFCLABEL)
    ProductionYear = "2026" (IFCLABEL)
  Pset_Recycled_EnvironmentalImpact | properties | on 1 object (1 IFCCOVERING)
    BiogenicCarbon_kgCO2_per_kg = -0.20000000000000001 (IFCREAL)
    DeclaredValueType = "estimated_literature" (IFCLABEL)
    EPDStatus = "literature_estimate" (IFCLABEL)
    EmbodiedEnergy_MJ_per_kg = 6.2000000000000002 (IFCREAL)
    GWP_kgCO2eq_per_kg = 0.55000000000000004 (IFCREAL)
    LCAModuleCoverage = "A1-A3" (IFCLABEL)
  Pset_Recycled_Hygrothermal | properties | on 1 object (1 IFCCOVERING)
    Porosity_percent = 70. (IFCREAL)
    SpecificHeatCapacity_J_per_kg_K = 1400. (IFCREAL)
    VapourDiffusionResistanceFactor_mu = 1.8 (IFCREAL)
  Pset_Recycled_Classifications | properties | on 1 object (1 IFCCOVERING)
    OmniClass_Code = "23-13 13 21" (IFCLABEL)
    OmniClass_Table = "23" (IFCLABEL)
    OmniClass_Title = "Acoustic Panels" (IFCLABEL)
    Uniclass2015_Code = "Pr_25_57_06" (IFCLABEL)
    Uniclass2015_Table = "Pr" (IFCLABEL)
    Uniclass2015_Title = "Acoustic boards and panels" (IFCLABEL)